****

**TYSONIC SPEAKER FLEX**

**PRODUCT SPECIFICATION**

**1.PRODUCT CODE** LMC04/2.1

**2. DESCRIPTION** 4 Core 105/.16 (2.1mm sq nom.) T.C.W. V75 P.V.C insulated.

 HBZRH-80FZW Low smoke, Low Halogen P.V.C. sheathed .

 Tysonic Speaker Flex.

 Oxygen free copper . RoHS compliant .

**3. CONSTRUCTION**

 **3.1 CONDUCTOR :** 105 strands of 0.16 mm Annealed Copper to

 AS/NZS1125 drawn from Class 102 copper to AS/NZS1574.

 Max. D.C. resistance at 20C : 8.6 ohms / km

 **3.2 INSULATION :** Coloured V75 PVC to AS/NZS3808

 Nominal Diameter : 2.65 mm

 Nom. Wall Thickness: 0.60 mm

 **3.3 LAY UP**  4 Cores.

 1. Red 2. Black 3. White 4. Green

 **3.4 SHEATH** Coloured P.V.C. type HBZRH-80FZW

 Nominal Diameter : 8.5 mm

 Nom. Wall Thickness : 1.0 mm

* 1. **IDENTIFICATION**

Printed at max 1000mm spacings

Cable to be meter marked, i.e every 1 meter

 TYCAB NZ Y.O.M. – 2.1mm² 14AWG 4 CORE 100V LINE SPEAKER CABLE M|M